# **PRESET MINIATURE REGULATOR FOR AIR**

**CartReg®**



# **CartReg®**

CartReg® - The economical and compact solution to various pneumatic applications. Engineered to comply with various international Health and Safety regulations on air blow guns, the preset CartReg® is the economical answer to keep in check the maximum pressure requirements. The preset miniature regulator is designed to meet OSHA (Occupational Safety & Health Administration, USA) and other safety agency requirements for 2 bar/30 psig maximum pressure for pneumatic air guns

The tamperproof the CartReg® can be easily mounted on any ¼” air blow gun and pneumatic tool and is an economical means to maintain the ideal pressure.

# **Your advantages**

* Safety: protects personnel, machinery and plant by avoiding pressure surges
* Ensures optimal air tool efficiency by supplying a constant pre-set pressure
* Prevents compressed air waste – limits excessive compressed air consumption = reducing energy costs
* Easy assembly: can be integrated into any ¼” pneumatic tool
* Lightweight (15g) and compact (Hexagon 14 mm, length 24 mm)
* Locked to prevent pressure change – tamper proof
* Competitively priced
* Increases tool service life

|  |  |  |  |
| --- | --- | --- | --- |
| **Technical data** |  | **Applications** |  |
| Max. inlet pressure: | 12 bar  | Pneumatic air gun | Spray gun |
| Outlet pressure (preset): | 2… 8 bar  | Workshop air lines | Pneumatic tools |
| Flow: | 350 Nl/min  | General pneumatic appl. |  |
| Connection: | 1/4" BSP/NPT |  |  |
| Temperature range: | -20°C to 60°C  |  |  |
| Weight: | 15g |  |  |



\*Dimensions see datasheet on website – protect-air.com



 

**TRI-MATIC AG
Bösch 82
CH-6331 Hünenberg**

**Phone +41 (0)41 780 22 22
Email: info@tri-matic.ch**

a brand of tri-matic